DUNES COMMUNITY DEVELOPMENT DISTRICT 

Plant capacity is currently 1,440,000 gallons per day.  It 

these tests that exceeded specifed criteria are included. 
We will notify you immediately if there is any reason for 
concern about our water. 

Tis report shows our water quality results and explains 
what they mean. It also provides important information 

	Te  following  information  is  provided  on  the  hardness 
Tis   interconnection   was   utilized   with   Palm   Coast    of the water: 

If  present,  elevated  levels  of  lead  can  cause  serious  health  problems,  especially  for  pregnant  women  and  young  children.    Lead 
in  drinking  water  is  primarily  from  materials  and  components  associated  with  service  lines  and  home  plumbing.    Dunes  CDD 
is  responsible  for  providing  high  quality  drinking  water  although,  does  not  control  the  variety  of  materials  used  in  plumbing 
components.  When  your  water  has  been  sitting  for  several  hours,  you  can  minimize  the  potential  for  lead  exposure  by  fushing 
your tap for 30 seconds to 2 minutes before using water for drinking or cooking. If you are concerned about lead in your water, you 
may wish to have your water tested.  Information on lead in drinking water, testing methods, and steps you can take to minimize 
exposure is available from the Safe Drinking Water Hotline or at http://www.epa.gov/safewater/lead 

MCLs are set at very stringent levels. To understand the possible health efects described for many regulated constituents, a person 
would  have  to  drink  2  liters  of  water  every  day  at  the  MCL  level  for  a  lifetime  to  have  a  one-in-a-million  chance  of  having  the  
described health efect. Some people may be more vulnerable to contaminants in drinking water than the general population. 
Immuno-compromised persons such as persons with cancer undergoing chemotherapy, persons who have undergone organ 
transplants,  people  with  HIV/AIDS  or  other  immune  system  disorders,  some  elderly,  and  infants  can  be  particularly  at 
risk  from  infections.  Tese  people  should  seek  advice  about  drinking  water  from  their  health  care  providers.  EPA/CDC 
guidelines on appropriate means to lessen the risk of infection by Cryptosporidium and other microbiological contaminants 
are available from the SAFE DRINKING WATER HOTLINE (1-800-426-4791). 

2018 Annual Drinking Water Quality Report 

	treatment, the water is aerated to remove dissolved gases, 
	carbon  dioxide  and  hydrogen  sulfde,  that  are  present  
about your water and how it relates to your health. Te   in  the  groundwater  but  are  not  removed  in  the  RO 
information  in  this  report  is  based  primarily  on  2018    process.    Chlorine  in  the  form  of  sodium  hypochlorite 
facts   and   fgures.   However,   the   U.S.   Environmental    (commonly  known  as  bleach)  is  used  for  disinfection 
Protection   Agency   (EPA)   does   not   require   us   to    purposes  and  to  maintain  a  chlorine  residual  in  the 
perform  all  tests  every  year.  When  necessary,  some    water distribution system.  Afer RO treatment, aeration 
data  was  obtained  from  prior  years.  As  directed  by  the    and   disinfection,   a   stabilization   process   is   utilized, 
agencies  that  regulate  our  industry,  only  values  from    adding  a  small  amount  of  minerals  and  alkalinity  to  

	improve water quality and compatibility with the water 
	distribution  system  components.      In  2018  the  Florida 
	Department    of    Environmental    Protection    (FDEP) 
	performed  a  Source  Water  Assessment  on  our  system.  
Te  Dunes  Community  Development  District  (Dunes    Te  assessment  was  conducted  to  provide  information 
CDD)  began  providing  customers  with  water  from  its    about  any  potential  sources  of  contamination  in  the 
reverse  osmosis  water  treatment  plant  on  August  15,    vicinity  of  our  wells.  Tere  are  fve  potential  sources  of 
2007  and  has  continued  to  do  so  throughout  2018.     contamination  identifed  for  this  system  with  a  low  to  

	moderate  levels  of  concern.    Te  assessment  results  are 
is  expected  that  this  capacity  will  meet  the  anticipated    available  on  the  FDEP  Source  Water  Assessment  and  
needs   of   the   community   at   build-out.   Te   Dunes    Protection Program website at 
www.dep.state.f.us/swapp. 
Palm  Coast  Utility  (PWS  ID#  2180863)  water  system 
for  emergencies  and  planned  maintenance  activities.  

Utility  supplying  water  during  the  period  of  February    Total Hardness: 
27   -   March   7,   2018   due   to   scheduled   maintenance    Calcium Hardness 
and  inspection  of  the  District’s  750,000  gallon  water  

45 ppm or 2.6 grains per gal. 
35 ppm or 2.0 grains per gal. 

storage  tank.    Te  Palm  Coast  Utility  Drinking  Water 
Quality  report  is  available  on  their  website  at  www. 
palmcoastgov.com. 

If you have any questions about this report or concerns 
about your water utility, please contact the Dunes CDD 
ofce  at  386-445-9045.  You  may  also  visit  the  Dunes 
www.dunescdd.org or cal 

Te Dunes CDD’s water treatment plant utilizes a reverse 
osmosis  (RO)  process  to  treat  a  brackish  groundwater 
supply withdrawn from three (3) Floridan Aquifer wells 
having  a  depth  of  300  f.    Te  RO  membrane  process 
removes  salts  and  minerals  from  the  water.    Afer  RO  

Drinking  Water  Hotline  at  1-800-426-4791.  We  want 
our valued customers to be informed about their water 
utility.  If  you  would  like  to  learn  more,  please  call  us  
for  information  about  the  next  opportunity  for  public 
participation in decisions about your drinking water. 

Likely Source o 

Lik 

and regulations. Except 

In  order  to  ensure  that  tap  water  is  safe  to  drink,  the  

(E)        Radioactive contaminants, which can be naturally 

including 

(C)      Pesticides and herbicides, which may come from a 

(A)      Microbial   contaminants,  such   as   viruses   and 

Maximum residual disinfectant level goal or MRDLG: 

Maximum  residual  disinfectant  level  or  MRDL:    Te    water  systems.    Te  Food  and  Drug  Administration  

Action Level (AL):  Te concentration of a contaminant 

Parts per billion (ppb) or Micrograms per liter (µg/l) 

Parts   per   million   (ppm)   or   Milligrams   per   liter   

Maximum  Contaminant  Level  Goal  or  MCLG:  Te                

Maximum  Contaminant  Level  or  MCL:  Te  highest  

It’s easy. Te table shows the results of our water-quality 

f 

e 

(FDA)  regulations  establish  limits  for  contaminants  in  

Te  level  of  a  drinking  water  disinfectant  below  which  

highest  level  of  a  disinfectant  allowed  in  drinking  water.  

(mg/l)  –  one  part  by  weight  of  analyte  to  1  million  parts    (D)    Organic     chemical     contaminants, 

level  of  a  contaminant  in  drinking  water  below  which                urban  stormwater  runof,  industrial  or  domestic 

level  of  a  contaminant  that  is  allowed  in  drinking  water.            

analyses. As you can see by the table, our system had no    Te  sources  of  drinking  water  (both  tap  water  and  

violations.  We’re proud that your water meets or exceeds    bottled  water)  include  rivers,  lakes,  streams,  ponds,  

all Federal and State requirements.  Te column marked    reservoirs,  springs,  and  wells.    As  water  travels  over  

	AL 
Exceeded 
	(Y/N) 

	Dates of 
sampling 
	(mo./yr.) 

	Contaminant and Unit 
 of Measurement 

 Radium 226 + 228 or combined 
	radium (pCi/L) 

Dates of sampling 
	(mo./yr.) 

last  time  tests  were  performed.  “Likely  Sources”  shows    dissolves  naturally  occurring  minerals  and,  in  some  

where  this  substance  usually  originates.  Descriptions  

not necessarily indicate that the water poses a health 

below explain other important details. In this table you 

risk.   More   information   about   contaminants   and   

may  fnd  unfamiliar  terms  and  abbreviations.  To  help    activity.  Contaminants  that  may  be  present  in  source  

potential health efects can be obtained by calling the 

you  better  understand  these  terms  we’ve  provided  the    water include: 

not refect the benefts of the use of disinfectants to control 

cases,  radioactive  material,  and  can  pick  up  substances  

    plants,    septic    systems,    agricultural    livestock 

            are    by-products    of    industrial    processes    and 

Environmental  Protection  Agency’s  Safe  Drinking  

i 

following defnitions: 

best available treatment technology. 

allow for a margin of safety. 

was not found by laboratory analysis.   

by weight of the water sample. 

of the water sample. 

in water. 

that a water system must follow. 

is necessary for control of microbial contaminants. 

microbial contaminants. 

DRINKING WATER? 

resulting  from  the  presence  of  animals  or  from  human  

           operations and wildlife. 

which  can  be  naturally-occurring  or  result  from 

           mining or farming. 

           stormwater runof and residential uses. 

           petroleum production, and can also come from gas 

           systems. 

           and mining activities. 

of  certain  contaminants  in  water  provided  by  public  

for public health. 

be  expected  to  contain  at  least  small  amounts  of  some  

Water Hotline at 1-800-426-4791. 

	period of 
January 1 to December 31, 2018 for the Dunes CDD - PWS ID # 2184259. Te Environmental Protection Agency 

Detected 

ge of 

 Source 

Detected 

 or 

nation 

HOW DO I READ THIS? 

WHAT  CAN  I  EXPECT  TO  FIND  IN  MY  

2018 ANNUAL DRINKING WATER QUALITY TEST RESULTS 

Dunes CDD routinely monitors for contaminants in your drinking water according to Federal and State laws, rules, 

where 

indicated otherwise, this 

report 

is 

based on the 

results of 

monitoring 

for 

the 

“Level  Detected”  shows  the  highest  results  from  the    the   surface   of   the   land   or   through   the   ground,   it   

(EPA) requires monitoring of over 80 drinking water contaminants. Tose contaminants listed in the table below are 
the only contaminants detected in your drinking water. 

Results in the Level Detected column for radioactive contaminants, inorganic contaminants, synthetic organic contaminants including pesticides and 

herbicides, and volatile organic contaminants are the highest average at any of the sampling points or the highest detected level at any sampling point, 
depending on the sampling frequency. 

Radioactive 
Contaminants 

MCLs  are  set  as  close  to  the  MCLGs  as  feasible  using  the  

                      bacteria,  which  may  come  from  sewage  treatment 

(B)     Inorganic contaminants, such as salts and metals, 

Contaminant and Unit of 
Measurement 

2/2017 
Inorganic Contaminants 

	MCL 
Violation 
	Y/N 
N 

Level Detected 

0.8 

Range 
	of 
Results 

MCLG 

0 

MCL 

5 

Likely Source of 
	Contamination 
Erosion of natural 
	deposits 

there  is  no  known  or  expected  risk  to  health.    MCLGs                   wastewater   discharges,   oil   and   gas   production, 

 Barium (ppm) 

2/2017 

N 

0.00038 

N/A 

2 

2 

		Discharge of drilling 
	wastes; discharge from 
metal refineries; erosion 
	of natural deposits 

 “ND” means not detected and indicates that the substance 

            variety   of   sources   such   as   agriculture,   urban 

Mercury (inorganic) (ppb) 

2/2017 

No 

0.018 

N/A 

2 

2 

		Erosion of natural 
	deposits; discharge 
	from refineries and 
factories; runoff from 
	landfills; runoff from 
		cropland 

               synthetic   and   volatile   organic   chemicals,   which 

 Sodium (ppm) 

2/2017 

N 

37 

N/A 

N/A 

160 

Salt water intrusion, 
	leaching from soil 

Stage 1 Disinfectants and Disinfection By-Products 

– one part by weight of analyte to 1 billion parts by weight                stations,   urban   stormwater   runof   and   septic 

For chlorine, the level detected is the the highest running annual average (RAA), computed quarterly, of monthly averages of all samples 
collected.   The range of results is the range of results of all the individual samples collected during the past year. 

Picocurie per liter (pCi/L) - measure of the radioactivity 

           occurring or be the result of oil and gas production 

Disinfectant or 
Contaminant and Unit of 
Measurement 

Dates of 
sampling 
(mo./yr.) 

MCL or 
	MRDL 
Violation 
	Y/N 

Level 

Ran 
Results 

MCLG or 
MRDLG 

MCL or 
MRDL 

ly 

of Contamination 

that, if exceeded, triggers treatment or other requirements 

Chlorine (ppm) 

01/2018 –  
	12/2018 

N 

1.30 

0.61 – 
	1.73 

MRDLG = 4 

MRDL = 4.0 

Water additive used to control 
	microbes 

EPA  prescribes  regulations,  which  limit  the  amounts  

Stage 2 Disinfectants and Disinfection By-Products 

During 2018, the system had only annual results and all of these results were below the MCL. 

Tere is convincing evidence that addition of a disinfectant 

bottled  water,  which  must  provide  the  same  protection  

Disinfectant or 
Contaminant and Unit of 
Measurement 

Dates of 
sampling 
(mo./yr.) 

MCL or 
	MRDL 
Violation 
	Y/N 

Level 

Range of 
Results 

MCLG or 
MRDLG 

MCL 
MRDL 

Contam 

Drinking water, including bottled water, may reasonably 

Haloacetic Acids (five) 
(HAA5) (ppb) 

07/2018 

N 

3.86 

NA 

NA 

MCL = 60 

By-product of drinking water 
	disinfection 

there is no known or expected risk to health.  MRDLGs do    contaminants.   Te  presence  of  contaminants  does  

 TTHM [Total 
Trihalomethanes] (ppb) 

07/2018 

N 

34.28 

NA 

NA 

MCL = 80 

By-product of drinking water 
	disinfection 

“N/A” means not applicable 

	90th 
Percentile 
	Result 
Lead and Copper (Tap Water) 

No. of sampling 
	sites exceeding 
	the AL 

MCLG 

	AL 
(Action 
	Level) 

Likely Source of Contamination 

Copper (tap water) 
(ppm) 

06//2018 
	– 
	07/2018 

N 

0.060 

0 

1.3 

1.3 

Corrosion of household plumbing systems; 
erosion of natural deposits; leaching from 
	wood preservatives 

 Lead (tap water) 
	(ppb) 

06//2018 
	– 
	07/2018 

N 

ND 

0 

0 

15 

Corrosion of household plumbing systems; 
	erosion of natural deposits