Contaminant and Unit of Measurement	Dates of
sampling (mo./yr.)	AL
Exceeded (Y/N)	90th
Percentile Result	No. of sampling
sites exceeding the AL	
MCLG	AL
(Action Level)	
Likely Source of Contamination	
Lead and Copper (Tap Water)	
Copper (tap water) (ppm)	06//2018
–    07/2018	
N	
0.060	
0	
1.3	
1.3	Corrosion of household plumbing systems; erosion of natural deposits; leaching from
wood preservatives	
Lead (tap water) (ppb)	06//2018
–    07/2018	
N	
ND	
0	
0	
15	Corrosion of household plumbing systems; erosion of natural deposits	

 	

If present, elevated levels of lead can cause serious health problems, especially for pregnant women and young children. Lead in drinking water is primarily from materials and components associated with service lines and home plumbing. Dunes CDD is responsible for providing high quality drinking water although, does not control the variety of materials used in plumbing components. When your water has been sitting for several hours, you can minimize

DUNES COMMUNITY DEVELOPMENT DISTRICT
2020 Annual Drinking Water Quality Report

the potential for lead exposure by flushing your tap for 30 seconds to 2 minutes before using water for drinking or cooking. If you are concerned about lead in your water, you may wish to have your water tested. Information on lead in drinking water, testing methods, and steps you can take to minimize exposure is available from the Safe Drinking Water Hotline or at http://www.epa.gov/safewater/lead

We are required to monitor your drinking water for specific contaminants on a regular basis. Results of regular monitoring are an indicator of whether or not your drinking water meets health standards. During the 2020 monitoring period, we did not monitor or test for a second set of Synthetic Organic Contaminants (SOCs), and therefore cannot be sure of the quality of your drinking water at that time. Some people who drink water containing Synthetic Organic Contaminants (SOCs) could become seriously ill. Health effects language for individual contaminants can be obtained by visiting the EPA website at https://www.epa.gov/ground-water-and-drinking-water-regulated-drinking-water-contaminants. Any customers who are concerned about their exposure to these contaminants can choose alternative sources of water for ingestion.  Replacement samples were taken for SOCs on February 2, 2021 and the sample results showed no detection of any contaminants.

MCLs are set at very stringent levels. To understand the possible health effects described for many regulated constituents, a person would have to drink 2 liters of water every day at the MCL level for a lifetime to have a one- in-a-million chance of having the described health effect. Some people may be more vulnerable to contaminants in drinking water than the general population. Immuno-compromised persons such as persons with cancer undergoing chemotherapy, persons who have undergone organ transplants, people with HIV/AIDS or other immune system disorders, some elderly, and infants can be particularly at risk from infections. These people should seek advice about drinking water from their health care providers. EPA/CDC guidelines on appropriate means to lessen the risk of infection by Cryptosporidium and other microbiological contaminants are available from the SAFE DRINKING WATER HOTLINE (1-800-426-4791).

This report shows our water quality results and explains what they mean. It also provides important information about your water and how it relates to your health. The information in this report is based primarily on 2020 facts and figures. However, the U.S. Environmental Protection Agency (EPA) does not require us to perform all tests every year. When necessary, some data was obtained from prior years. As directed by the agencies that regulate our industry, only values from these tests that exceeded specified criteria are included. We will notify you immediately if there is any reason for concern about our water.

The Dunes Community Development District (Dunes CDD) began providing customers with water from its reverse osmosis water treatment plant on August 15, 2007 and has continued to do so throughout 2020.  Plant capacity is currently 1,440,000 gallons per day.  It is expected that this capacity will meet the anticipated needs of the community at build-out. The Dunes CDD currently maintains an interconnection with the Palm Coast Utility (PWS ID# 2180863) water system for emergencies and planned maintenance activities. The interconnection was activated, and Palm Coast Utility water was supplied during the period of August 10 – 12, 2020 for a scheduled shutdown and replacement of electrical equipment at the water treatment plant. The Palm Coast Utility Drinking Water Quality Report is available on their website at www.palmcoastgov.com.

The Dunes CDD’s water treatment plant utilizes a reverse osmosis (RO) process to treat a brackish groundwater supply withdrawn from three (3) Floridan Aquifer wells having a depth of 300 ft.  The RO membrane process removes salts and minerals from the water.  After RO treatment, the water is aerated to remove dissolved gases, carbon dioxide and hydrogen sulfide, that are present in the groundwater but are not removed in the RO process.  Chlorine in the form of 

sodium hypochlorite (commonly known as bleach) is 
used for disinfection purposes and to maintain a chlorine residual in the water distribution system.  After RO treatment, aeration and disinfection, a stabilization process is utilized, adding a small amount of minerals and alkalinity to improve water quality and compatibility with the water distribution system components.   In 2019 the Florida Department of Environmental Protection (FDEP) performed a Source Water Assessment on our system. The assessment was conducted to provide information about any potential sources of contamination in the vicinity of our wells. There are five unique and potential sources of groundwater contamination identified for this system all having a low level of concern.  The assessment results are available on the FDEP Source Water Assessment and Protection Program website at www.dep.state.fl.us/swapp. 

The following information is provided on the hardness of the water:
Total Hardness:	45 ppm or 2.6 grains per gal.
Calcium Hardness	35 ppm or 2.0 grains per gal.

If you have any questions about this report or concerns about your water utility, please contact the Dunes CDD office at 386-445-9045. You may also visit the Dunes CDD website at www.dunescdd.org or call the EPA Safe Drinking Water Hotline at 1-800-426-4791. We want our valued customers to be informed about their water utility. If you would like to learn more, please call us for information about the next opportunity for public participation in decisions about your drinking water. 

HOW DO I READ THIS?

It’s easy. The table shows the results of our water- quality analyses. As you can see by the table, our system had no violations. We’re proud that your water

meets or exceeds all Federal and State requirements. The column marked “Level Detected” shows the highest results from the last time tests were performed. “Likely Sources” shows where this substance usually originates. Descriptions below explain other important details. In this table you may find unfamiliar terms and abbreviations. To help you better understand these terms we’ve provided the following definitions:

Maximum Contaminant Level or MCL: The highest level of a contaminant that is allowed in drinking water. MCLs are set as close to the MCLGs as feasible using the best available treatment technology.

Maximum Contaminant Level Goal or MCLG: The level of a contaminant in drinking water below which there is no known or expected risk to health. MCLGs allow for a margin of safety.

“ND” means not detected and indicates that the substance was not found by laboratory analysis.

Parts per million (ppm) or Milligrams per liter (mg/l) – one part by weight of analyte to 1 million parts by weight of the water sample.

Parts per billion (ppb) or Micrograms per liter (μg/l) – one part by weight of analyte to 1 billion parts by weight of the water sample.

Picocurie per liter (pCi/L) - measure of the radioactivity in water.

Action Level (AL): The concentration of a contaminant that, if exceeded, triggers treatment or other requirements that a water system must follow.

Maximum residual disinfectant level or MRDL: The highest level of a disinfectant allowed in drinking water. There is convincing evidence that addition of a disinfectant is necessary for control of microbial contaminants.

Maximum residual disinfectant level goal or MRDLG: The level of a drinking water disinfectant below which there is no known or expected risk to health. MRDLGs do not reflect the benefits of the use of disinfectants to control microbial contaminants.

“N/A” means not applicable

WHAT CAN I EXPECT TO FIND IN MY DRINKING WATER?

The sources of drinking water (both tap water and bottled water) include rivers, lakes, streams, ponds, reservoirs, springs, and wells. As water travels over the surface of the land or through the ground, it dissolves naturally occurring minerals and, in some cases, radioactive material, and can pick up substances resulting from the presence of animals or from human activity. Contaminants that may be present in source water include:

(A)	Microbial contaminants, such as viruses and bacteria, which may come from sewage treatment plants, septic systems, agricultural livestock operations, and wildlife.

(B)	Inorganic contaminants, such as salts and metals, which can be naturally-occurring
or result from urban stormwater runoff, industrial or domestic wastewater discharges, oil and gas production, mining, or farming.

(C)	Pesticides and herbicides, which may come from a variety of sources such as agriculture, urban stormwater runoff, and residential uses.

(D)	Organic chemical contaminants, including synthetic and volatile organic chemicals, which are by-products of industrial processes and petroleum production, and can also come
from gas stations, urban stormwater runoff, and septic systems.

(E)	Radioactive contaminants, which can be naturally occurring or be the result of oil and gas production and mining activities.

In order to ensure that tap water is safe to drink, the EPA prescribes regulations, which limit the amounts of certain contaminants in water provided by public water systems. The Food and Drug Administration (FDA) regulations establish limits for contaminants in bottled water, which must provide the same protection for public health.

Drinking water, including bottled water, may reasonably be expected to contain at least small amounts of some contaminants. The presence of contaminants does not necessarily indicate that the water poses a health risk. More information about contaminants and potential health effects can be obtained by calling the Environmental Protection Agency’s Safe Drinking Water Hotline at 1-800-426-4791.

2020 ANNUAL DRINKING WATER QUALITY TEST RESULTS
Dunes CDD routinely monitors for contaminants in your drinking water according to Federal and State laws, rules, and regulations. Except where indicated otherwise, this report is based on the results of monitoring for the period of January 1 to December 31, 2020 for the Dunes CDD - PWS ID # 2184259. The Environmental Protection Agency (EPA) requires monitoring of over 80 drinking water contaminants. Those contaminants listed in the table below are the only contaminants detected in your drinking water.

Results in the Level Detected column for radioactive contaminants, inorganic contaminants, synthetic organic contaminants including pesticides and herbicides, and volatile organic contaminants are the highest average at any of the sampling points or the highest detected level at any sampling point, depending on the sampling frequency	
Radioactive Contaminants	
Contaminant and Unit of Measurement	Dates of sampling (mo./yr.)	MCL Violation Y/N	Level Detected	Range of Results	MCLG	MCL	Likely Source of Contamination	
 Radium 226 + 228 or combined radium (pCi/L)	2/2017	N	0.8		0	5	Erosion of natural deposits	
Inorganic Contaminants	
Sodium (ppm)	2/2020	N	47	N/A	N/A	160	Saltwater intrusion, leaching from soil	

Stage 1 Disinfectants and Disinfection By-Products	
 For chlorine, the level detected is the the highest running annual average (RAA), computed quarterly, of monthly averages of all samples        collected.  The range of results is the range of results of all the individual samples collected during the past year.	
Disinfectant or Contaminant and Unit of Measurement	Dates of sampling (mo./yr.)	MCL or MRDL Violation Y/N	Level Detected	Range of Results	MCLG or MRDLG	MCL or MRDL	Likely Source of Contamination	
Chlorine (ppm)	01/2020 – 
12/2020	N	1.06	0.58 – 1.70	MRDLG = 4	MRDL = 4.0	Water additive used to control microbes	

Stage 2 Disinfectants and Disinfection By-Products	
 During 2020, the system had only annual results and all of these results were below the MCL.
	
Disinfectant or Contaminant and Unit of Measurement	Dates of sampling (mo./yr.)	MCL or MRDL
Violation
Y/N	
Level
Detected	
Range of Results	
MCLG or MRDLG	
MCL or MRDL	
Likely Source of Contamination	
 
Haloacetic Acids (five) (HAA5) (ppb)	07/2020	N	3.54	NA	NA	MCL = 60	By-product of drinking water disinfection	
 TTHM [Total Trihalomethanes] (ppb)	07/2020	N	31.30	NA	NA	MCL = 80	By-product of drinking water disinfection